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The following minimum construction inspections are required as indicated in Part I of the Virginia Uniform Statewide Building Code (VUSBC). These inspections are the typical minimum inspections for standard type construction projects, but may not be all inclusive or may not be applicable in all cases. Inspections, such as, Braced Wall Line( 606), may be requested prior to a complete rough-in inspection in order to install house wrap/flashing, etc.. Inspection numbers are not necessarily in the order in which they are constructed.  If in doubt, call Stafford County Department of Public Works @ 540-658-8650 for assistance. All inspections must be scheduled & passed, prior to concealment. Please call 540-658-4151 to schedule inspections using the Stafford County Interactive Voice Response (IWR) system or the Integrated Web Response system (IWR) or (HELLO) system on the Stafford County Code Administration website. If a required inspection is unavailable for scheduling under the automated system, you must call the permit office for assistance. Inspections can be scheduled by any interested party but the ultimate responsibility for ensuring all inspections have been completed lies with the permit holder (VUSBC 113.1.2).
Inspections will not be made if the following minimum requirements have not been met:
1. Street or lot must be identified (VUSBC 110.5).
2. Permit must be posted on site, visible from street (VUSBC 110.5).
3. Original (red stamped) approved plan must be on site for all inspections (VUSBC 109.5).
4. Any ladder, scaffolding or test equipment must be provided by the permit holder (VUSBC 113.1.1).
New Homes
	Inspection Type
	Inspection Code

	First Erosion
	100

	Final Erosion
	199

	Footing/House
	200

	Waterproofing (drain tile)
	202

	Foundation Wall 
	203

	Slab/Porch/Patio
	204 (as applicable)

	Footing/Garage/Carport
	206 (as applicable)

	Footing/Deck/Porch
	207 (as applicable)

	Stoop
	208

	Slab/On Grade/Basement
	210 (as applicable)

	Slab/Garage/Carport/Barn
	211 (as applicable)

	Wall Preparation (stamped, approved site plan with walk out location shown)


	213



	Area-way stairs/slab
	218



	Soils Certification
	261

	Plumbing/Rough-in
	300

	Plumbing Groundwork’s
	301

	Plumbing/Water Line
	302

	Plumbing/Sewer Line
	303

	Permanent Water Meter Set
	305

	Mechanical/Rough-in
	400

	Mechanical/Gas Line/Inside
	401 (as applicable)

	Mechanical/Tanks/Propane/Oil
	402 (as applicable)

	Mechanical/Gas Line/Outside
	403

	Insert/Thimble/Woodstove
	405 (as applicable)

	Fireplace/Prefab/Reline (Instruction manual on site; do not include unit shut off valve in pressure test)
	408 (as applicable)

	Fireplace/Hearth
	409 (as applicable)

	Fireplace/Throat
	411 (as applicable)

	Electric/Rough-in
	500

	Electric/Meter Permanent 
	501

	Electric/Steel & Bonding/Ufer
	502

	Site Trenching/Conduit/Residential


	503



	Electric Sub-panel
	504

	Framing


	600



	Energy 
	601

	Insulation
	602

	Braced Wall Line/Wind Bracing


	606



	Waterproof Membrane/Flashing( 2006 code)
	607

	Fire Wall/Separation
	660( as applicable)

	Final (Building & Trades)
	999


	Operational Permit for well and septic system or verification of connection to public utilities required for Certificate of Occupancy


MINIMUM REQUIRED RESIDENTIAL INSPECTIONS BY PROJECT











Page 2 of 11

